SECTION 062522

WOOD WALL PANELING

(Quartile 1 and Quartile 2 by Spinneybeck)

1. GENERAL
   * + 1. DESCRIPTION OF WORK
          1. Work Included: Provide labor, materials and equipment necessary to complete the work of this Section including the following.

Wall-mounted wood panels.

* + - * 1. Related Work: The following items are not included in this Section and are specified under the designated Sections:

Section 061000 - Rough Carpentry; concealed blocking and supports.

* + - 1. SUBMITTALS
         1. Product Data: Submit for each product indicating materials, dimensions, profiles, textures and colors. Include installation instructions.
         2. Shop Drawings: Submit shop drawings indicating plans, elevations, details of construction, and relationship with adjacent construction.
         3. Verification Samples: Submit representative sample in material and finish specified.
      2. QUALITY ASSURANCE
         1. Manufacturer: Minimum of 2 years manufacturing similar products.
         2. Installer: Minimum of 2 years installing similar products.
      3. DELIVERY, STORAGE, AND HANDLING
         1. Delivery: Deliver materials in manufacturer’s original, unopened, undamaged containers with identification labels intact.
         2. Storage and Handling: Comply with manufacturer's recommendations for storage and handling. Protect from weather damage.
      4. WARRANTY
         1. Warranty: Provide manufacturer's standard limited warranty against defects in manufacturing.

1. PRODUCTS
   * + 1. MANUFACTURER
          1. Manufacturer: Spinneybeck, 425 CrossPoint Parkway, Getzville, NY 14068. Tel 800.482.7777, 716.446.2380. Fax 716.446.2396. sales@spinneybeck.com, www.spinneybeck.com.
       2. WOOD WALL PANELING
          1. Basis-of-Design: [Quartile 1] [Quartile 2] by Spinneybeck.

Designer: Lars Beller Fjetland.

Tile Size: 1’-0” x 1’-0” (30.5 x 30.5 cm)

Tile Size Tolerance: +/- 1/16 inch (2 mm).

Thickness: 1 inch (2.5 cm).

Wood Type: [Beech] [Douglas Fir] [Maple] [Sapele] [Walnut] [White oak] solid wood.

Grain Direction: Vertical.

Edges: Finished.

Color: 1 color per wall.

Custom Color: 2-color+ per wall.

Durability: Contract or residential.

Variation: Wood is a natural material and minor changes in color are evidence of the 100% natural origin of the material.

Environmental: Contains no formaldehyde, CARB compliant, solid woods inherently non-emitting.

Flammability: Solid woods meet ASTM E 84, Class A (with applied fire retardant) and CAN ULC S101.2-18: FS: 20 / SDI: 95-105 (with applied fire-retardant).

Heavy-Duty Construction Adhesive: As recommended by manufacturer.

1. EXECUTION
   * + 1. EXAMINATION
          1. Examine existing conditions to determine that they are suitable for installation. Proceed with installation only when unsatisfactory conditions have been corrected.
       2. INSTALLATION
          1. Clean substrates of projections and substances detrimental to application.
          2. Adhere tiles to substrate in accordance with manufacturer's instructions, approved submittals, and in proper relationship to adjacent construction.
       3. ADJUSTING AND CLEANING
          1. Adjust units for proper position and uniform appearance. Clean exposed and semi-exposed surfaces using materials acceptable to manufacturer.
          2. Maintenance: Use a very mild non-abrasive, non-ammonia, and non-alcohol containing soap diluted in a room temperature water solution. Apply with a soft flannel cloth, followed by a dry cloth. Always wipe in the direction of the grain. Do not use commercial cleaners, abrasives, solvents, or glass cleaner on any wood components as it will wear away the finish. Do not apply wax as this will interact with the finish.

END OF SECTION